
Running on Linux
----------------

To enable the editor to talk to the modules via USB Serial on Linux you will have to add some rules to udev to enable this.

See https://www.pjrc.com/teensy/49-teensy.rules for details.

Then launch the editor via the ProkModularProcessingApp.jar file.
